****

**Conductive thread**

|  |  |  |
| --- | --- | --- |
| https://github.com/ecraft2learn/OER/blob/master/conductive%20thread/Conductive%20thread.jpg?raw=true | A little thicker than every day thread, but still thin enough to be sewn in medium-eye needles or with a sewing machine that can handle "heavy" thread.   |  | | --- | | **It is ideal for any wearable/e-textile project. It is made of stainless steel fibers, thus your projects will not "stop working" because of oxidation after a few months and its safe to wash.** |   In [Conductive Thread - 10 tips](https://www.youtube.com/watch?v=XT5ygUt8Cbk) you get inspiration for your project! |

   [Licença Creative Commons](http://creativecommons.org/licenses/by-nc/4.0/)